**Features**

Powerful, fuel-injected, 4-stroke engine is easy on gas

Large fuel tank and plush seat deliver extended, comfortable riding range

Fender-mounted shifter controls the QuadMatic™ transmission

Select 2WD or 4WD via a handlebar-mounted lever

Metallic Matte Rocky Gray bodywork complements the cast aluminum wheels with highlighted spokes and rim edges

The KingQuad 400ASi SE+’s fuel-injected 376cc four-stroke, four-valve engine produces efficient power and driveablity.

Suzuki's class-leading fuel injection smooths power output, especially in the mid-to-high range, and provides excellent cold starting. The system uses 3-D maps for optimum ignition, creating responsive yet environmentally compliant performance.

Suzuki Advanced Cooling System (SACS) uses an oil cooler and thermostat-controlled cooling fan to shed engine heat during hard work or cargo hauling.

Push-button electric starting has a start-in-gear function allowing starting without shifting to neutral (as conditions permit).

The Engine Control Unit (ECU) has slip control logic, which adjusts fuel injector duration and timing to improve drivability and grip in loose/slippery conditions.

Highly efficient iridium spark plug contributes to better combustion, cleaner emissions, and longer plug life. Engine starting under low temperature is also improved.

Pulsed-secondary AIR-injection (PAIR) system and catalyst-equipped exhaust system help the ATV comply with Environmental Protection Agency (EPA) emission standards while maintaining a high level of performance. The QuadMatic™ transmission is a fully automatic, CVT (continuously variable transmission) with selectable high/low sub-transmission and reverse for maximum traction and fuel efficiency.

Automotive gate-type gearshift lever lets you conveniently choose high or low range, neutral, or reverse.

Select 2WD and 4WD with the flip of a handlebar-mounted lever. The shaft drive system is reliable and durable and is nearly maintenance-free.

Torque-sensing limited-slip front differential provides maximum traction and light steering when in 4WD mode.

An advanced engine-braking system minimizes free-wheeling with the throttle off to help control the ATV during descents.

The ECU has a Reverse Mode that monitors vehicle speed so higher engine RPM can be used when getting out of mud or loose soil in reverse mode.

Sporty bodywork features sharply angled, high-clearance fenders finished in a unique, Metallic Matte Rocky Gray color.

Suzuki's plush T-shaped seat delivers rider mobility during sport or difficult terrain riding. Overall length is under 82 inches (208 cm), so the KingQuad fits into a 6.5-foot truck bed for easy transportation.

Independent front A-arm suspension offers smooth performance and remarkable ground clearance with 6.7 inches (170.1 mm) of wheel travel.

A swingarm rear suspension with 6.7 inches (170.1 mm) of wheel travel and twin shock absorbers provides agile handling and plush riding.

Dual front hydraulic disc brakes feature calipers with large, 34mm pistons and wide brake-pad surface area for increased stopping power and outstanding durability. Lightweight and strong plastic skid plates are sturdy to withstand trail pounding, yet slippery to let obstacles slide below.

Lightweight and strong plastic skid plates are sturdy to withstand trail pounding, yet slippery to let obstacles slide below.

Large, 25-inch Carlisle tires with aggressive tread offer consistent traction in wet conditions, yet make for a quiet, smooth ride on hard-packed trails.

Cast aluminum wheels are powder-coated black so they complement the metallic gray bodywork.

Dual 35-watt headlights (with high and low settings) are part of the distinctive KingQuad grille appearance. Bright taillight helps make the ATV visible in dark conditions.

Heavy-duty front and rear cargo racks let you take advantage of the ATV’s superb load capabilities. Wrinkle paint finish on the racks and front bumper is durable and scratch resistant.

LCD instrumentation includes speedometer, odometer, trip meter, hour meter, clock, fuel gauge and indicators for reverse, neutral, oil and FI (fuel injection).

Automotive-style DC power outlet is included on front fender.

Winch-ready mounts and wire conduit make winch installation simple.

Large, 4.2 gallon (16.0 L) fuel tank provides outstanding riding range.

Full floorboards with integrated raised footpegs provide protection. 12-month limited warranty. Longer coverage periods with other benefits available through Suzuki Extended Protection (SEP).\*  
  
\*Subject to separate coverage for certain parts and the exclusions and limitations described in the New ATV Limited Warranty.

A variety of Suzuki Genuine Accessories are available, including winches, windshield, front and rear bumpers, snowplow, aluminum skid pans, rack extensions, utility box, and more.